**BLE Message definition**

**SERVICE\_DATA**

1. Battery data + NTC 10K data + LDR data + Contact data

Code: 0x0004

Package:

Battery data 2B

NTC 10K data 2B

LDR data 2B

Contact data 1B

Example:

uint8\_t service\_data[9];

service\_data[0] = 0x00;

service\_data[1] = 0x04;

service\_data[2] = (uint8\_t) ((batData>>8) & 0xff);

service\_data[3] = (uint8\_t) (batData & 0xff);

service\_data[4] = (uint8\_t) ((ntcData>>8) & 0xff);

service\_data[5] = (uint8\_t) (ntcData & 0xff);

service\_data[6] = (uint8\_t) ((ldrData>>8) & 0xff);

service\_data[7] = (uint8\_t) (ldrData & 0xff);

service\_data[8] = (uint8\_t) (dorData & 0xff);